**List of Available workflow script command for "Hawkeye Core"**

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Syringe Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!SyringeCmd SyringeInitializeCmd

S, I

!SyringeCmd SetValveCmd SetToPortParam DirectionParam(0 : Clockwise)

S, V, 2, 1

!SyringeCmd SetSyringeMoveCmd TargetVolumeParam SpeedParam

S, M, 500, 600

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Camera Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!CameraCmd SetGainCmd GainParam

C, G, 30

!CameraCmd TakePictureCmd LedTypeParams GainParam ExposureParam

C, T, 1, 30, 50

!CameraCmd ABICmd SyringeVolParam SyringeRateParam CameraExposureParam LedTypeParams TargetIntensityParam OffSetParam

C, ABI, 500, 600, 50, 1, 135, 2

!CameraCmd CameraCaptureCmd SyringeVolParam SyringeRateParam CameraExposureParam LedTypeParams NumImageParam NumWarmupImageParam

C, C, 500, 600, 50, 1, 10, 5

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Focus Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!FocusCmd FocusHomeCmd

F, H

!FocusCmd FocusAutoCmd LedTypeParams CameraExposureParam

F, A, 1, 50

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***LED Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!LedCmd SetLedParam LedTypeParams %PowerParam SimmerCurrentVoltageParam ltcdParam ctldParam feedbackPhotodiodeParam

L, S, 0, 0, 0, 0, 0, 0

!LedCmd UseParam

L [BRIGHTFIELD][TOP\_1][BOTTOM\_1][TOP\_2][BOTTOM\_2]

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Reagent Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!ReagentCmd ReagentParamUpCmd

R, U

or R, 0

!ReagentCmd ReagentParamDownCmd

R, D

or R, 1

!ReagentCmd ReagentParamPurgeCmd

R, P

or R, 2

!ReagentCmd ReagentParamDoorCmd

R, L

or R, 3

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Directory Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!DirectoryCmd PathParam

D, "x:\path\_to\_directory"

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Wait Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!WaitCmd WaitMilisecParam

W, 2000

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Workflow State Changed Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

!StateChangeCmd CurrentStateParam

SC, 3

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Run Script Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

! RunScriptCmd PathToScriptParam

N, “folder\path-toscript.txt”

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***Flow Control Commands**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

! RepetitionsCmd NumCmdsToRepeat RepetitionCount

! Repeats the next NumCmdsToRepeat commands a total of RepetitionCount times

! If RepetitionCount is NUMERIC, then it is taken as a literal ('3', '100', etc).

! if RepetitionCount begins with a non-numeric character, then it is taken as a   
! reference to a software-supplied label

! Current labels: “mixing\_cycles”, “aspiration\_cycles”

! Repeat next 3 commands a number of times supplied by the software:

REPEAT, 3, mixing\_cycles

! Repeat next 2 commands a total of 5 times:

REPEAT, 2, 5

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/